[COMMON]	 	
PRODUCT_LANGUAGE=EN
COMPANY_NAME=Mercury
PROGRAM_FOLDER_NAME=Mercury
BASE_FOLDER_NAME=Program Files\Mercury
;	 	
USBHUB_NAME=Mercury P2760
SCANNER_NAME=Mercury P2760 SCAN
PRINTER_NAME=OEP3050DN
DRV_MDL_NAME=OEP3050DN
PORT_NAME=USB001
;	 	
VID_PID=VID_356C&PID_0042
USB_SERIAL=0000000000000000
PNP_LPT=Mercury_P27600FC9
PNP_USB=Mercury_P2760
PNP_CHECKSUM=0FC9
USB_PARENT_ID=6&26dc5742&0&0001
;	 	
BUTTON_OK=OK
BUTTON_CANCEL=Cancel
MSG_ERR_CAPTION=Error!!!
MSG_FILE_NOT_FOUND=The system cannot find the file specified.
MSG_DIR_NOT_FOUND=The system cannot find the path specified.
MSG_FILE_NOT_OPEN=The system cannot open the file.
MSG_SHARING_VIOLATION=The process cannot access the file because it is being used by another process.
MSG_FILE_SIZE_ZERO=The file size is 0 byte.
MSG_ACCESS_DENIED=Access is denied.
MSG_HANDLE_INVALID=The handle is invalid.
MSG_ERROR_CODE=Error code:
	 	
[WEBSITE]	 	
default=
current=
	 	
[SETMAN]	 	
CAPTION=Reference Guide Setup
PRODUCT_NAME=Mercury P2760 Reference Guide
UNINSTALL_NAME=Mercury P2760 Reference Guide
SHORTCUT_NAME=Mercury P2760 Reference Guide
ICON_NAME=PRIX903.ICO
PRODUCT_KEY_FILE=M1XXE0HL.HLP
UNINSTALL_KEY_FILE=M1SETMAN.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Reference Guide and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
	 	
[SETSTM]	 	
CAPTION=Status Monitor Setup
PRODUCT_NAME=Mercury P2760 Status Monitor
UNINSTALL_NAME=Mercury P2760 Status Monitor
SHORTCUT_NAME=Mercury P2760 Status Monitor
ICON_NAME=PRIX902.ICO
PRODUCT_KEY_FILE=M1XXE0SM.EXE
UNINSTALL_KEY_FILE=M1SETSTM.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Status Monitor and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
;	 	
TITLE_STM=Mercury Monitor 3
;	 	
InTitle=Mercury Printer Utility Setup
InEND=Mercury Status Monitor Setup is complete.
;	 	
UnTitle=Mercury Printer Utility Uninstall
UnEND=Uninstall complete.
;	 	
URLSET1=Choose the country or region in which you use this printer.
URLSET2=By choosing a country or a region, you will activate the online consumables order function.
URLSET3=Consumables Web Site URL:
;	 	
WEB1=Korea
WEB2=(No Setting)
URL1=http://www.iprix.co.kr/
URL2=
;	 	
msgChange=You have changed the URL. Do you want to keep the new setting?
;	 	
	 	
[SETDRV]
IPHONENUMBER=88165526
TELEPHONENUMBER=1234 	
CAPTION=Printer Driver Setup
GROUP_NAME=Mercury P2760
PRODUCT_NAME=Mercury P2760 Printer Driver
UNINSTALL_NAME=Mercury P2760 Printer Driver
SHORTCUT_NAME=Mercury P2760 Printer Driver
ICON_NAME=PRIX901.ICO
PRODUCT_KEY_FILE=M1XXE0DR.DLL
UNINSTALL_KEY_FILE=M1SETDRV.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Printer Driver and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
;	 	
; progress dialog	 	
;	 	
CAPTION_INSTALL=Copying files...
CAPTION_UNINSTALL=Deleting files...
;	 	
INF_OEMx=oem0.inf
INF_SEC_LPT=OEM_LPT
INF_SEC_USB=OEM_USB
INF_SEC_MFG=OEM_MFG
INF_MFG=Mercury
INF_DATE=01-02-2006
LANG_MONITOR=P2760 Language Monitor
PORT_MONITOR=USBMON
DATA_TYPE=RAW
SHARE_NAME=P2760
;	 	
PATH_LANGUAGE=English
PATH_WIN9X=WIN9X
PATH_WINXP_2K=WINXP_2K
;	 	
PAPER_USERDEFINED=User Defined Size
	 	
[MESSAGE]	 	
MSG_REG_UPDATE=<<< Changing Registry ... >>>
;	 	
MSG_FILE_NOT_FOUND=File not found
;	 	
MSG_EXECUTE_ERROR=Execute Error
MSG_WIN_9X=This program requires Windows 98/98SE/ME.
MSG_WIN_NT=This program requires Windows NT 4.0.
MSG_WIN_XP=This program requires Windows 2000/XP/2003.
;	 	
MSG_END_INST=Mercury P2760 software was installed.
MSG_END_UNINST=Mercury P2760 software was uninstalled.
	 	
[FILENAME]	 	
;	 	
; Driver (XP)	 	
;	 	
FN_DRV2K_DLL=M1XXE0DR.DLL
FN_DRV2K_GPD=M1XXE0DR.GPD
FN_DRV2KUI_DLL=M1XXE0UI.DLL
FN_DRV2KHT_DLL=M1XXE0HT.DLL
FN_DPINST_EXE=DPINST.EXE
;	 	
; Uni-Driver (XP)	 	
;	 	
;FN_STDNAMES_GPD=STDNAMES.GPD
;FN_UNIDRV_DLL=UNIDRV.DLL
;FN_UNIDRV_HLP=UNIDRV.HLP
;FN_UNIDRVUI_DLL=UNIDRVUI.DLL
;FN_UNIRES_DLL=UNIRES.DLL
;	 	
; Driver (9x)	 	
;	 	
FN_DRV9X_DRV=M1XXE1DR.DRV
FN_DRV9X_DLL=M1XXE2DR.DLL
;	 	
; Driver (ALL)	 	
;	 	
FN_STMRSP_DAT=M1XXE0SM.DAT
FN_DRV_HLP=M1XXE0HL.HLP
FN_DRVIMAGE_DLL=M1XXE0IP.DLL
FN_DRVPRINT_DLL=M1XXE0PS.DLL
FN_MDLIMAGE_BMP=M1XXE1PS.BMP
FN_LEDLIGHT_BMP=M1XXE2PS.BMP
FN_LANGMON_DLL=M1XXE0LM.DLL
FN_LANGSEND_DLL=M1XXE0SP.DLL
FN_JBIG_EXE=M1XXE0JB.EXE
FN_MSGBOX_DLL=M1XXE0MB.DLL
FN_RUNCHECK_EXE=M1XXE0RC.EXE
FN_DRVRES_DAT=M1XXEDRV.DAT
;	 	
; Status Monitor	 	
;	 	
FN_SETSTM_EXE=M1SETSTM.EXE
FN_SETSTM_DAT=M1SETSTM.DAT
FN_STM_EXE=M1XXE0SM.EXE
;	 	
; CD Run	 	
;	 	
FN_AUTORUN_INF=AUTORUN.INF
FN_CDROM_ICO=CDROMLP.ICO
FN_CDSETUP_EXE=CDSETUP.EXE
;	 	
; Setup (Install, Uninstall)	 	
;	 	
FN_SETDRV_EXE=M1SETDRV.EXE
FN_SETDRV_DAT=M1SETSET.DAT
FN_SETUNE_EXE=M1SETUNE.EXE
FN_SETUNE_EXE=M1XXE0DF.EXE
FN_SETLINK_EXE=M1SETLNK.EXE
;	 	
; Setup (Add Printer)	 	
;	 	
FN_DRV9X_INF=M1XXE0ME.INF
FN_DRV2K_INF=M1XXE0XP.INF
FN_DRV2K_CAT=M1XXE0XP.CAT
FN_DRV2K_INI=M1XXE0DR.INI
FN_SETVENDOR_DLL=M1SETVND.DLL
;	 	
; Setup (PnP)	 	
;	 	
FN_USBHUB_INF=M1XUSBHU.INF
FN_USBHUB_SYS=USBHUB.SYS
FN_USBPRINT_INF=M1XUSBPR.INF
FN_USBPRINT_SYS=USBPRINT.SYS
FN_USBMON_DLL=USBMON.DLL
FN_USBSCAN_INF=M1XUSBSC.INF
FN_USBSCAN_CAT=M1XUSBSC.CAT
FN_USBSCAN_SYS=USBSCAN.SYS
;	 	
; Manual	 	
;	 	
FN_SETMAN_EXE=M1SETMAN.EXE
FN_SETMAN_DAT=M1SETMAN.DAT
	 	
[FW_MSG]	 	
V_READY=Printer is ready
V_READYi1=Printer is ready.
V_PRINTING=printing
V_PRINTINGi1=please waiting...
V_CANCEL=print job deleted
V_CANCELi1=memory forced reset
V_WARMINGUP=Warming Up
V_WARMINGUPi1=please waiting...
V_POWER_SAVE=Power saving mode
V_POWER_SAVEi1=This mode is canceled automatically when printing is performed
;V_POWER_SAVEi1=This mode is canceled automatically when printing is performed
V_PRT_OTHER_PORT=Printing data from another port
;V_PRT_OTHER_PORT=Printing data from another port
V_PRT_OTHER_PORTi1=please waiting...
;V_PRT_OTHER_PORTi1=Please wait.
V_INCOR_PAPER_WR=No black cartridge kit
;V_INCOR_PAPER_WR=Printing on incorrect paper size
V_INCOR_PAPER_WRi1=Please input black cartridge kit
;V_INCOR_PAPER_WRi1=Select the correct size paper.
V_NOT_ALL_PRINT=Toner is insufficient
;V_NOT_ALL_PRINT=Toner is insufficient
V_NOT_ALL_PRINTi1=Toner is insufficient
;V_NOT_ALL_PRINTi1=This error might be avoided by selecting Avoid Insufficient Memory Error in Extended Settings on the printer driver's Optional Settings menu.
V_CONSUM_N_END=Consumables near end of service life
;V_CONSUM_N_END=Consumables near end of service life
V_CONSUM_N_ENDi1=Prepare the following consumables:
;V_CONSUM_N_ENDi1=Prepare the following consumables:
V_CONSUM_N_ENDi2=Drum Kit
;V_CONSUM_N_ENDi2=Process Cartridge Unit
V_CONSUM_N_ENDi3=Toner Kit
;V_CONSUM_N_ENDi3=Toner Kit
V_N_END_TONER=Black toner kit near end of service life
;V_N_END_TONER=Toner Kit near end of service life
V_N_END_TONERi1=Please change black cartridge.
;V_N_END_TONERi1=Prepare a new Toner Kit.
V_N_END_OPC=Process Cartridge Unit near end of service life
;V_N_END_OPC=Process Cartridge Unit near end of service life
V_N_END_OPCi1=Prepare a new Process Cartridge Unit.
;V_N_END_OPCi1=Prepare a new Process Cartridge Unit.
V_N_GENUINE_INST=Non-genuine Toner Kit installed
;V_N_GENUINE_INST=Non-genuine Toner Kit installed
V_N_GENUINE_INSTi1=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
;V_N_GENUINE_INSTi1=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_CONSUM_WARNING=Consumables warning
;V_CONSUM_WARNING=Consumables warning
V_CONSUM_WARNINGi1=Prepare the following consumables:
;V_CONSUM_WARNINGi1=Prepare the following consumables:
V_CONSUM_WARNINGi2=Drum Kit
;V_CONSUM_WARNINGi2=Process Cartridge Unit
V_CONSUM_WARNINGi3=Toner Kit
;V_CONSUM_WARNINGi3=Toner Kit
V_CONSUM_WARNINGi4=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended
;V_CONSUM_WARNINGi4=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_N_END_NONTONER=Toner Kit near end of service life
;V_N_END_NONTONER=Toner Kit near end of service life
V_N_END_NONTONERi1=Prepare a new drum
;V_N_END_NONTONERi1=Prepare a new Process Cartridge Unit.
V_N_END_NONTONERi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended
;V_N_END_NONTONERi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_TOO_MUCH_DATA=Data decoding error
;V_TOO_MUCH_DATA=Page contains too much data to process
V_TOO_MUCH_DATAi1=Data decompression error, please stop printing.
V_NO_MEMORY=Insufficient memory
;V_NO_MEMORY=Insufficient memory
V_NO_MEMORYi1=Click Continue to resume printing
;V_NO_MEMORYi1=Click Continue to resume printing.
V_NO_MEMORYi2=Click Continue to resume printing
;V_NO_MEMORYi2=Click Cancel Printing to cancel the print job.
V_SIZE_TYPE_ERR=Black cartridge does not match
;V_SIZE_TYPE_ERR=Incorrect paper size
V_SIZE_TYPE_ERRi1=Please change drum kit
;V_SIZE_TYPE_ERRi1=The paper size selected in the printer driver does not match the paper size that is loaded.
V_SIZE_SET_ERR=Incorrect paper size
;V_SIZE_SET_ERR=Incorrect paper size
V_SIZE_SET_ERRi1=Please check the paper size and reload paper
;V_SIZE_SET_ERRi1=The paper size selected in the printer driver does not match the paper size that is loaded.
V_FATAL_ERROR=Paper jam at back
V_FATAL_ERRORi1=Please open front cover or take out the cassette, then remove any jammed paper

V_PAPER_READY=Paper ready
V_PAPER_READYi1=Paper ready
V_DOCUM_READY=Manuscript ready
V_DOCUM_READYi1=Manuscript ready

V_OPC_MISSING=No drum kit!
V_OPC_MISSINGi1=Please install drum kit.
V_OPC_MISSINGi2=
V_OPC_MISMATCH=Drum kit does not match!
V_OPC_MISMATCHi1=Please replace drum.
V_OPC_MISMATCHi2=
V_OPC_RONOUT=Drum kit is at the end of service life!
V_OPC_RONOUTi1=Please replace drum.
V_OPC_RONOUTi2=
V_OPC_LESS=Drum kit near end of service life!
V_OPC_LESSi1=Please check the drum kit.
V_OPC_LESSi2=

V_COVER_OPEN=Front cover open.
;V_COVER_OPEN=Top cover open
V_COVER_OPENi1=Close front cover.
;V_COVER_OPENi1=Close the cover.
V_JAM_PRINT=Paper jam at the front of the mechanism
;V_JAM_PRINT=Paper jam - printer
V_JAM_PRINTi1=Please take out the cassette, then remove any jammed paper.
;V_JAM_PRINTi1=Open the top and output covers, then remove any jammed paper.
V_JAM_PRINT_002=Paper jam in the middle of the printer.
;V_JAM_PRINT_002=Paper jam - printer
V_JAM_PRINT_002i1=Open the front cover, take out the drum, then remove any jammed paper.
;V_JAM_PRINT_002i1=Open the top and output covers, then remove any jammed paper.
V_JAM_PRINT_003=Paper jam at the back of the mechanism.
;V_JAM_PRINT_003=Paper jam - printer
V_JAM_PRINT_003i1=Open the back covers and fixing unit, then remove any jammed paper.
;V_JAM_PRINT_003i1=Open the top and output covers, then remove any jammed paper.
V_FEED_JAM=Paper jam in manual tray
;V_FEED_JAM=Unable to feed paper
V_FEED_JAMi1=Open front cover, take out the drum, then remove any jammed paper.
;V_FEED_JAMi1=Reload the paper.
V_FEED_JAM_PAP=Paper jam at the output.
;V_FEED_JAM_PAP=Unable to feed paper
V_FEED_JAM_PAPi1=Open the back covers and fixing unit, then remove any jammed paper.
;V_FEED_JAM_PAPi1=Open the cover.
V_JAM_OUTPUT=Paper jam - output
;V_JAM_OUTPUT=Paper jam - output
V_JAM_OUTPUTi1=Open back cover, then remove any jammed paper.
;V_JAM_OUTPUTi1=Open the top and output covers, then remove any jammed paper.
V_OUTPUT_C_OPEN=Output cover open.
;V_OUTPUT_C_OPEN=Output cover open
V_OUTPUT_C_OPENi1=Close output cover.
;V_OUTPUT_C_OPENi1=Close the cover.
V_TONER_OUT_ERR=Back cover open.
;V_TONER_OUT_ERR=Toner out
V_TONER_OUT_ERRi1=Close back cover.
;V_TONER_OUT_ERRi1=Close the cover.
*%V_TONER_OUT_ERRi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
*%;V_TONER_OUT_ERRi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_NO_CARTRIGE=Black toner insufficient
;V_NO_CARTRIGE=Toner Kit not installed
V_NO_CARTRIGEi1=Please check black cartridge
;V_NO_CARTRIGEi1=Toner Kit not installed
V_TONER_ID_ERR=Paper jam at manual tray
;V_TONER_ID_ERR=Incorrect Toner Kit
V_TONER_ID_ERRi1=Please take out the cassette, open the manual tray, then remove any jammed paper
;V_TONER_ID_ERRi1=Open the top cover, then remove and reinstall the Toner Kit.
V_TONER_RW_ERR=Paper feeding failed.
;V_TONER_RW_ERR=Trouble with Toner Kit
V_TONER_RW_ERRi1=Please check the tray
;V_TONER_RW_ERRi1=Open the top cover, then reinstall or replace the Toner Kit.
V_NGENUINE_TONER=Paper jam at the manual tray
;V_NGENUINE_TONER=Non-genuine toner
V_NGENUINE_TONERi1=Please check manual tray, then remove any jammed paper.
;V_NGENUINE_TONERi1=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_GENERAL_ERROR=General error
;V_GENERAL_ERROR=General error
V_GENERAL_ERRORc2=Error No.:%s
;V_GENERAL_ERRORc2=Error No.:%s
V_GENERAL_ERRORi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
;V_GENERAL_ERRORi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
V_GENERAL_ERRORi2=If this error occurs again, contact your dealer.
;V_GENERAL_ERRORi2=If this error occurs again, contact your dealer.

V_TEMP_ERROR_001=Warming error.
V_TEMP_ERROR_001i1=Please restart the printer.

V_PRINTING_HOT=ADC heat error.
V_PRINTING_HOTi1=Please restart the printer.
V_TEMP_ERROR_002=Overheating
V_TEMP_ERROR_002i1=Please wait for hear dissipation.
V_LSU_ERROR_001=External humidity sensor error.
V_LSU_ERROR_001i1=Turn off the printer and wait a few minutes before turning it on. If the error still occurs, please contact your dealer.


V_KLSU_ERROR_001=Black laser synchronization error.
V_KLSU_ERROR_001i1=No synchronization signal received. Turn off the printer and wait a few minutes before turning it on.
V_KLSU_ERROR_001i2=If the error still occurs, please contact your dealer.

V_KLSU_ERROR_002=Black laser motor error.
V_KLSU_ERROR_002i1=No ready signal received. Turn off the printer and wait a few minutes before turning it on.
V_KLSU_ERROR_002i2=If the error still occurs, please contact your dealer.


V_PRT_INTERRUPT=Error in data format.
;V_PRT_INTERRUPT=Printing interrupted
V_PRT_INTERRUPTi1=Command parsing error, please stop printing.
;V_PRT_INTERRUPTi1=Check the cassette
V_PRT_INTERRUPTING=Data receiving time out.
;V_PRT_INTERRUPTING=Printing interrupted
V_PRT_INTERRUPTINGi1=please stop printing.
;V_PRT_INTERRUPTINGi1=Check the cassette
V_ERR_OTHER_PC=Error occurred while printing data from another computer
;V_ERR_OTHER_PC=Error occurred while printing data from another computer
V_ERR_OTHER_PCi1=Please wait until the error is cleared.
;V_ERR_OTHER_PCi1=Please wait until the error is cleared.
V_OTHER_PC_PRINT=Printing the different document.
;V_OTHER_PC_PRINT=Printing the different document
V_OTHER_PC_PRINTi1=Printing the different document.
;V_OTHER_PC_PRINTi1=Please wait until printing is finished.
V_ERR_OTHER_PORT=Error occurred while printing data from another port.
;V_ERR_OTHER_PORT=Error occurred while printing data from another port
V_ERR_OTHER_PORTi1=Please wait until the error is cleared.
;V_ERR_OTHER_PORTi1=Please wait until the error is cleared.
V_UNKNOWN_ERROR=Unknown error
;V_UNKNOWN_ERROR=Unknown error
V_UNKNOWN_ERRORi1=Check the printer.
;V_UNKNOWN_ERRORi1=Check the printer.
V_COMM_ERROR=Communication error
;V_COMM_ERROR=Communication error
V_COMM_ERRORi1=Check all cable connections and make sure the printer is on.
;V_COMM_ERRORi1=Check all cable connections and make sure the printer is on.
V_S_CONFIRM_ERR=Status confirmation error
;V_S_CONFIRM_ERR=Status confirmation error
V_S_CONFIRM_ERRi1=Check all cable connections and make sure the printer is on.
;V_S_CONFIRM_ERRi1=Check all cable connections and make sure the printer is on.
V_S_CONFIRM_ERRi2=This message can appear when a print job takes a long time to process. This message clears when printing finishes.
;V_S_CONFIRM_ERRi2=This message can appear when a print job takes a long time to process. This message clears when printing finishes.
V_S_CONFIRM_ERRi3=Check the printer status to make sure printing has not stopped due to another error.
;V_S_CONFIRM_ERRi3=Check the printer status to make sure printing has not stopped due to another error.
V_DIFF_DEVICE=Different device from specified
;V_DIFF_DEVICE=Different device from specified
V_DIFF_DEVICEi1=Attempting to connect to a different device from that specified in the driver. Check the driver and the device.
;V_DIFF_DEVICEi1=Attempting to connect to a different device from that specified in the driver. Check the driver and the device.
V_SEARCHING=Searching...
;V_SEARCHING=Searching
V_SEARCHINGi1=Please wait....
;V_SEARCHINGi1=Please wait.
V_C1_FEED_JAM=Unable To Feed Paper In Cassette1
;V_C1_FEED_JAM=Unable To Feed Paper In Cassette1
V_C1_FEED_JAMi1=Check the cassette
;V_C1_FEED_JAMi1=Check the cassette.
V_C2_FEED_JAM=Unable To Feed Paper In Cassette2
;V_C2_FEED_JAM=Unable To Feed Paper In Cassette2
V_C2_FEED_JAMi1=Check the cassette
;V_C2_FEED_JAMi1=Check the cassette.
V_C3_FEED_JAM=Unable To Feed Paper In Cassette3
;V_C3_FEED_JAM=Unable To Feed Paper In Cassette3
V_C3_FEED_JAMi1=Check the cassette
;V_C3_FEED_JAMi1=Check the cassette.
V_CIS_FAIL=Scan positive position failed
V_CIS_FAILi1=Scan positive position failed
V_CAP_OPEN=Scanner upper cover open
V_CAP_OPENi1=Please close the upper cover of the scanner
V_ADF_JAM=Card draft
V_ADF_JAMi1=Clear the paper
V_TOO_LONG=The manuscript is too long
V_TOO_LONGi1=Please select the appropriate manuscript size.
V_NO_DOC=No manuscript 
V_NO_DOCi1=Please put the manuscript into the scanner
V_NO_LOAD=Citation failure
V_NO_LOADi1=Reput the manuscript 
V_NO_EJECT=Rrjection failed
V_NO_EJECTi1=Please clear the manuscript.
V_GET_JAM_PAP=Paper jam - printer
;V_GET_JAM_PAP=Paper jam - printer
V_GET_JAM_PAPi1=Check the cassette.
;V_GET_JAM_PAPi1=Check the cassette.
V_FEED_JAM_PA=Paper jam at the input port.
;V_FEED_JAM_PA=Unable to feed paper
V_FEED_JAM_PAi1=Open front cover, take out the drum, then remove any jammed paper.
;V_FEED_JAM_PAi1=Reload the paper.
V_MTRAY_JAM=Paper jam at tray.
V_MTRAY_JAMi1=Please take out the cassette, open the manual tray, then remove any jammed paper.

V_DRUM_END=Drum end of life
;V_DRUM_END=Drum end of life
V_DRUM_ENDi1=Open the top cover, then replace the drum unit.
;V_DRUM_ENDi1=Open the top cover, then replace the drum unit.
V_INCORRECT_MEDI=Incorrect media type
;V_INCORRECT_MEDI=Incorrect media type
V_INCORRECT_MEDIi1=Please check the paper size and reload paper.
;V_INCORRECT_MEDIi1=The media type selected in the printer driver does not match the media type that is loaded.
V_LETTLE_ERROR=Low toner.
;V_LETTLE_ERROR=Fatal error
V_LETTLE_ERRORi1=红色墨粉少
;V_LETTLE_ERRORi1=Fatal error
V_CST_N_PAPER=No Paper
;V_CST_N_PAPER=No Paper
V_CST_N_PAPERi1=Please put the paper.
;V_CST_N_PAPERi1=Supply the paper in manual tray.
V_MAN_N_PAPER=No Paper in manual tray.
;V_MAN_N_PAPER=No Paper
V_MAN_N_PAPERi1=Supply the paper in manual tray.
;V_MAN_N_PAPERi1=Supply the paper in manual tray.
*%V_MAN_N_PAPERi2=To print with other media type, please select the manual feed mode and put paper in munual feed tray.
*%;V_MAN_N_PAPERi1=Supply the paper in manual tray.
V_AUTO_N_PAPER=Paper feeding error.
;V_AUTO_N_PAPER=Misfeed
V_AUTO_N_PAPERi1=Check the paper in cassette or manual tray.
;V_AUTO_N_PAPERi1=Check the paper in cassette or manual tray.
V_AUTO_N_PAPERi2=Open and close the cover.
;V_AUTO_N_PAPERi2=Open and close the cover.
V_PRINTER_BUSY=Printer is busy.
;V_PRINTER_BUSY=Printer is busy.
V_PRINTER_BUSYi1=Please wait...
;V_PRINTER_BUSYi1=Please wait.
V_TEST_MODE=Test mode
;V_TEST_MODE=Test mode
V_TEST_MODEi1=Please wait until the test mode is cleared.
;V_TEST_MODEi1=Please wait until the test mode is cleared.
V_TEST_MODE_ERR=Test mode error
;V_TEST_MODE_ERR=Test mode error
V_TEST_MODE_ERRi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
;V_TEST_MODE_ERRi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
V_CST1_N_PA=Paper Out Cassette1
;V_CST1_N_PA=Paper Out Cassette1
V_CST1_N_PAi1=Supply the paper in cassette tray.
;V_CST1_N_PAi1=Supply the paper in cassette tray.
V_CST2_N_PA=Paper Out Cassette2
;V_CST2_N_PA=Paper Out Cassette2
V_CST2_N_PAi1=Supply the paper in cassette tray.
;V_CST2_N_PAi1=Supply the paper in cassette tray.
V_CST3_N_PA=Paper Out Cassette3
;V_CST3_N_PA=Paper Out Cassette3
V_CST3_N_PAi1=Supply the paper in cassette tray.
;V_CST3_N_PAi1=Supply the paper in cassette tray.
V_OPC_N_END=Process Cartridge Unit near end of service life
;V_OPC_N_END=Process Cartridge Unit near end of service life
V_OPC_N_ENDi1=Prepare a new Process Cartridge Unit.
;V_OPC_N_ENDi1=Prepare a new Process Cartridge Unit.
V_TONER_N_END=Toner Kit near end of service life
;V_TONER_N_END=Toner Kit near end of service life
V_TONER_N_ENDi1=Prepare a new Toner Kit.
;V_TONER_N_ENDi1=Prepare a new Toner Kit.
V_PRINT_FAILURE=Print Failure
;V_PRINT_FAILURE=Print Failure
V_PRINT_FAILUREi1=Printing was not successful since a data for one page was not saved due to an insufficient memory.
;V_PRINT_FAILUREi1=Printing was not successful since a data for one page was not saved due to an insufficient memory.
V_PRINT_FAILUREi2=Click Close to resume printing the next page.
;V_PRINT_FAILUREi2=Click Close to resume printing the next page.
V_INSTALL_TONER=Install New Toner Cartridge
;V_INSTALL_TONER=Install New Toner Cartridge
V_INSTALL_TONERi1=Please wait...
;V_INSTALL_TONERi1=Please wait.

V_C1NOT_IN_PL=Cassette1 Not In Place
;V_C1NOT_IN_PL=Cassette1 Not In Place
V_C1NOT_IN_PLi1=Check the cassette tray
;V_C1NOT_IN_PLi1=Check the cassette tray
V_C2NOT_IN_PL=Cassette2 Not In Place
;V_C2NOT_IN_PL=Cassette2 Not In Place
V_C2NOT_IN_PLi1=Check the cassette tray
;V_C2NOT_IN_PLi1=Check the cassette tray
V_C3NOT_IN_PL=Cassette3 Not In Place
;V_C3NOT_IN_PL=Cassette3 Not In Place
V_C3NOT_IN_PLi1=Check the cassette tray
;V_C3NOT_IN_PLi1=Check the cassette tray
V_RTNOT_IN_PL=ReverseTray Not In Place
;V_RTNOT_IN_PL=ReverseTray Not In Place
V_RTNOT_IN_PLi1=Check the cassette tray
;V_RTNOT_IN_PLi1=Check the cassette tray
V_PAPER_LESS=Paper Less
;V_PAPER_LESS=Paper Less
V_PAPER_LESSi1=Input More Paper
;V_PAPER_LESSi1=Input More Paper

V_ENDOFMESSAGE=End of Message
;V_ENDOFMESSAGE=End of Message
V_ENDOFMESSAGEi1=Quit
;V_ENDOFMESSAGEi1=Quit.


V_FINGER_OK=指纹操作成功
V_FINGER_FAIL=指纹操作失败
V_FINGER_NEEDSWEEP=请输入指纹
V_FINGER_ERRORIDENTIFY=该指纹不存在
V_FINGER_TEMPLATEEMPTY=无指纹输入
V_FINGER_TEMPLATENOTEMPTY=选中的指纹不为空
V_FINGER_ALLTEMPLATEEMPTY=无存储指纹
V_FINGER_EMPTYIDNOEXIST=指纹存储已满
V_FINGER_DUPLICATIONID=该指纹已存在
V_FINGER_BADQUALITY=指纹图像质量不好
V_FINGER_TIMEOUT=指纹操作超时
V_FINGER_FPCANCEL=取消指纹操作
V_FINGER_INVALIDTEMPNO=选中的指纹不存在
V_FINGER_IDENTIFYSUCCESS=指纹识别成功
V_FINGER_REGISTERSUCCESS=注册指纹成功
V_FINGER_REGISTERFAIL=注册指纹失败
V_FINGER_DELETESINGLESUCCESS=指纹删除成功
V_FINGER_DELETEALLSUCCESS=全部指纹均已删除
V_FINGER_DELETEFAIL=删除指纹失败
V_FINGER_NEEDRELEASE=请离开手指
V_FINGER_UARTERROR=指纹模块通讯错误
V_FINGER_IDENTIFYSUCCESSi1=

	 	
 	
[PI_MSG]	 	
;	 	
; status sheet	 	
;	 	
SS100mfg=OEP3050DN
;SS100mfg=Mercury
SS100=Printer Information
;SS100=Printer Information
SS101=Printer Name
;SS101=Printer Name
SS102=Title
;SS102=Title
SS103=Printer Setting
;SS103=Printer Setting
SS104=Sleep Mode
;SS104=Sleep Mode
SS105=Cassette Paper size
;SS105=Cassette Paper size
SS106=Toner Out Error
;SS106=Toner Out Error
SS107=Total Pages
;SS107=Total Pages
SS108=Installed Memory
;SS108=Installed Memory
SS109=Communication Mode
;SS109=Communication Mode
SS110=High Speed
;SS110=High Speed
SS111=Full Speed
;SS111=Full Speed
SS112=Toner
;SS112=Toner
SS113=Part Number
;SS113=Part Number
SS114=Process Cartridge
;SS114=Process Cartridge
SS115=Part Number
;SS115=Part Number
SS116=Needed Soon
;SS116=Needed Soon
SS117=Lights
;SS117=Lights
SS117a=Paper Out, Paper Jam, Cover Open, and other errors.
;SS117a=Paper Out, Paper Jam, Cover Open, and other errors.
SS117b=Check Status Monitor 3 for details.
;SS117b=Check Status Monitor 3 for details.
SS117c=Toner Out and other errors.
;SS117c=Toner Out and other errors.
SS117d=Check Status Monitor 3 for details.
;SS117d=Check Status Monitor 3 for details.
SS117e=Warming Up, Receiving Data.
;SS117e=Warming Up, Receiving Data.
SS117f=Consumables Near End of Service Life and other warnings.
;SS117f=Consumables Near End of Service Life and other warnings.
SS117g=Check Status Monitor 3 for details
;SS117g=Check Status Monitor 3 for details.

SS117h=Other light patterns:
;SS117h=Other light patterns:
SS117i=See your printer's documentation or Status Monitor 3 for details.
;SS117i=See your printer's documentation or Status Monitor 3 for details.
SS118=Information
;SS118=Information
SS118a=Non-genuine cartridge installed. Using a non-genuine cartridge may affect print quality
;SS118a=Non-genuine cartridge installed. Using a non-genuine cartridge may affect print quality.
SS118b=Genuine Mercury cartridge recommended
;SS118b=Genuine Mercury cartridge recommended.
SS119=Controller Firmware Date
;SS119=Controller Firmware Date
SS120=Jam Counter
;SS120=Jam Counter
SS121=Counter of changing of toner
;SS121=Counter of changing of toner
SS122=Counter of changing of non-genuine toner
;SS122=Counter of changing of non-genuine toner
SS123=Engine Firmware Version
;SS123=Engine Firmware Version
SS124=USB ID
SS125=Consumables
;SS125=Consumables
SS130=CORPORATION
;SS130=PRIX CORPORATION
SS131=Min
;SS131=Min
SS132=Pages
;SS132=Pages
SS133=MB
;SS133=MB
	 	
[DI_MSG]	 	
;	 	
; Setting Information	 	
;	 	
SI200mfg=OEP3050DN
;SI200mfg=Mercury
;SI200=驱动程序信息
SI200=Driver Information
;SI201=布局
SI201=Layout
;SI202=定向
SI202=Orientation
;SI203=肖像
SI203=Portrait
;SI204=风景
SI204=Landscape
;SI205=打印顺序
SI205=Page Order
;SI206=从前到后
SI206=Front to Back
;SI207=从后到前
SI207=Back to Front
;SI208=每张打印页数
SI208=Pages Per Sheet
;SI209=页
SI209=pages
;SI210=打印结构
SI210=Print the Frame
;SI211=打印顺序
SI211=Print Order
;SI212=纸张/质量
SI212=Paper/Quality
;SI213=纸张来源
SI213=Paper Source
;SI214=纸张类型
SI214=Media
;SI215=高级
SI215=Advanced
;SI216=纸张/输出
SI216=Paper/Output
;SI217=纸张尺寸
SI217=Paper Size
;SI218=份数
SI218=Copy Count
;SI219=比较
SI219=Collated
;SI220=图形
SI220=Graphic
;SI221=打印分辨率
SI221=Print Quality
;SI222=文档选项
SI222=Document Options
;SI223=高级打印功能
SI223=Advanced printing features
;SI224=半色调
SI224=Halftoning
SI225=Image processing
;SI225=Brightness
;SI226=剩余墨粉量
SI226=Toner Save
;SI227=缩放选项
SI227=Zoom Options
;SI228=输出纸张
SI228=Output Paper
;SI229=缩放到
SI229=Zoom To
;SI230=缩放比例
SI230=Zoom Ratio
;SI231=位置
SI231=Location
;SI232=180度旋转
SI232=Rotate by 180
;SI233=可选设置
SI233=Optional Settings
;SI234=扩展设置
SI234=Extended Settings
;SI235=边距
SI235=Offset
;SI236=顶边距
SI236=Top Offset
;SI237=左边距
SI237=Left Offset
;SI238=跳过空白页
SI238=Skip Blank Page
;SI239=忽视选择的纸张尺寸
SI239=Ignore the selected paper size
;SI240=使用应用软件中指定的设置
SI240=Uses the collate settings specified in the application
;SI241=忽视内存溢出错误
SI241=Avoid Insufficient Memroy Error
;SI242=自动继续
SI242=Auto Continue
;SI243=监视打印状态
SI243=Monitor the printing status
;SI244=扩展的可打印区域
SI244=Extended Printable Area
;SI245=从打印服务器添加纸张尺寸
SI245=Add the paper size provided by the print server
;SI251=其他设置
SI251=Other Options
;SI252=海报打印
SI252=Poster Printing
;SI253=双面打印
SI253=Double-Sided Printing
;SI254=信纸头
SI254=Letterhead
;SI254a=布置
SI254a=Placement
;SI254b=文本
SI254b=Text
;SI254c=字体
SI254c=Font
;SI254d=大小
SI254d=Size
;SI254e=下划线
SI254e=Underline
;SI254f=加粗
SI254f=Bold
;SI254g=斜体
SI254g=Italic
;SI254h=失败
SI254h=Strikeout
;SI255=水印
SI255=Watermark
;SI255a=布置
SI255a=Placement
;SI255b=文本
SI255b=Text
;SI255c=字体
SI255c=Font
;SI255d=尺寸
SI255d=Size
;SI255e=颜色
SI255e=Color
;SI255f=强度
SI255f=Intensity
;SI255g=下划线
SI255g=Underline
;SI255h=加粗
SI255h=Bold
;SI255i=斜体
SI255i=Italic
;SI255j=边距
SI255j=Offset
;SI255k=角度
SI255k=Angle
;SI256=点数
SI256=Points	 	
[ITEM]	 	
;-----< >-----	 	
iv700=用户定义尺寸...
;-----< >-----	 	
iv701=Off
iv702=On
iv703=每天一次
;-----< >-----	 	
iv706=Disable
iv707=Enable
;-----< Paper Size >-----	 	
iv711=A4 210 x 297 mm
iv712=A3 297 x 420 mm
iv713=A5 148 x 210 mm
iv714=B4 257 x 364 mm
iv715=B5 182 x 257 mm
iv716=LT 8.5 x 11 in
iv717=HLT 5.5 x 8.5 in
iv718=LGL 8.5 x 14 in
iv719=GLT 8 x 10.5 in
iv720=GLG 8.5 x 13 in
iv721=B 11 x 17 in
iv722=EXE 7.25 x 10.5 in
iv723=F4 210 x 330 mm
iv724=16K 195 x 270 mm
;--- for World Wide Version ---	 	
iv725=MON 3.875 x 7.5 in
iv726=C10 4.125 x 9.5 in
iv727=DL 110 x 220 mm
iv728=C5 162 x 229 mm
iv729=C6 114 x 162 mm
iv730=IB5 176 x 250 mm
;--- for Japanese Version ---	 	
iv731=J O Postcard 100 x 148 mm
iv732=J W Postcard 148 x 200 mm
iv733=J 4-sided Postcard 200 x 296 mm
iv734=Youkei #0 120 x 135 mm
iv735=Youkei #4 105 x 135 mm
iv736=Youkei #6 98 x 190 mm
iv737=Choukei #3 120 x 235 mm
iv738=Kakukei #3 216 x 277 mm
;--- Common Paper ---	 	
iv739=A3F 311.2 x 457.2 mm
iv740=A3Wide 328 x 453 mm
iv741=FREE
iv742=FREE
iv743=FREE
iv744=FREE
iv745=FREE
iv746=FREE
iv747=FREE
iv748=FREE
iv749=FREE
iv750=FREE
iv751=FREE
iv752=FREE
iv753=FREE
iv754=FREE
iv755=FREE
iv756=FREE
iv757=FREE
iv758=FREE
iv759=User Defined Size
iv760=User Defined Size (Min)
iv761=User Defined Size (Max)
;-----< Paper Size (short) >-----	 	
iv711s=A4
iv712s=A3
iv713s=A5
iv714s=B4
iv715s=B5 (JIS)
iv716s=Letter
iv717s=Half Letter
iv718s=Legal
iv719s=Govt-Letter
iv720s=Govt-Legal
iv721s=B
iv722s=Executive
iv723s=F4
iv724s=C16K
;--- for World Wide Version ---	 	
iv725s=Envelope Monarch
iv726s=Envelope #10
iv727s=Envelope DL
iv728s=Envelope C5
iv729s=Envelope C6
iv730s=ISO B5
;--- for Japanese Version ---	 	
iv731s=J O Postcard
iv732s=J W Postcard
iv733s=J 4-sided Postcard
iv734s=Youkei #0
iv735s=Youkei #4
iv736s=Youkei #6
iv737s=Choukei #3
iv738s=Kakukei #3
;--- Common Paper ---	 	
iv739s=A3F
iv740s=A3 Wide
iv741s=FREE
iv742s=FREE
iv743s=FREE
iv744s=FREE
iv745s=FREE
iv746s=FREE
iv747s=FREE
iv748s=FREE
iv749s=FREE
iv750s=FREE
iv751s=FREE
iv752s=FREE
iv753s=FREE
iv754s=FREE
iv755s=FREE
iv756s=FREE
iv757s=FREE
iv758s=USER
iv759s=USER(Min)
iv760s=USER(Max)
;-----< Paper Source >-----	 	
iv761=Auto
iv762=Cassette
iv763=Manual Tray
;-----< Paper Type >-----	 	
iv771=Plain
iv772=Thick-Wide
iv773=Thick-Narrow
;-----< >-----	 	
iv781=1
iv782=2
iv783=4
iv784=6
iv785=9
iv786=16
;-----< Resolution >-----	 	
iv791=600x600 dpi
iv792=300x300 dpi
iv793=1200x600 dpi
iv794=1200x1200 dpi
;-----< Dithering >-----	 	
iv795=None
iv796=Smooth
iv797=Normal
iv798=Sharp
;-----< Brightness >-----	 	
iv801=None
iv802=Light
iv803=Lighter
iv804=Normal
iv805=Darker
iv806=Dark
;-----< Zoom Location >-----	 	
iv811=Upper Left
iv812=Center
;-----< Style >-----	 	
iv813=Ordinary
iv814=Scan
;-----< >-----	 	
iv821=Off
iv822=5 min
iv823=15 min
iv824=30 min
iv825=60 min
iv826=120 min
iv827=180 min
iv828=240 min
;-----< >-----	 	
iv831=A4
iv832=信纸
;-----< >-----	 	
iv833=Continue
iv834=Stop
;-----< >-----	 	
iv835=Reset
iv836=Set

[DLG_MSG]
T113=Other Settings
T122=About
I1247=Image Processing
I1251=Rotate by 180°
;	 	
; ---------- End of File ----------	 	
;	 	
